PATUAKHALI SCIENCE AND TECHNOLOGY UNIVERSITY

A logo of a university

Description automatically generated**Assignment Name: Lab Problem 16**

**Course Code: CCE-314**

**Course Title: Computer Networks Sessional**

Submitted by:

**Arfan Ahmed**

ID No.: 2002040

Registration No.: 09557

Level-3, Semester-1, Session: 2020-2021

Faculty of Computer Science & Engineering

Submitted to:

**Dr. Md. Samsuzzaman**

Professor

Department of Computer and Communication Engineering

Faculty of Computer Science and Engineering

Date of Submission: June 26, 2024

Lab - Calculate IPv4 Subnets (Instructor Version)

**Instructor Note**: Red font color or gray highlights indicate text that appears in the instructor copy only.

# Objectives

Part 1: Determine IPv4 Address Subnetting

Part 2: Calculate IPv4 Address Subnetting

# Background / Scenario

The ability to work with IPv4 subnets and determine network and host information based on a given IP address and subnet mask is critical to understanding how IPv4 networks operate. The first part is designed to reinforce how to compute network IP address information from a given IP address and subnet mask. When given an IP address and subnet mask, you will be able to determine other information about the subnet.

**Instructor Note**: This activity can be done in class or assigned as homework. If the assignment is done in class, you may wish to have students work alone or in teams of 2 students each. It is suggested that the first problem is done together in class to give students guidance as to how to proceed for the rest of the assignment.

The public IP addresses used in this lab are owned by Cisco.

# Required Resources

* 1 PC (Windows with Internet access)
* Optional: IPv4 address calculator

# Instructions

Fill out the tables below with appropriate answers given the IPv4 address, original subnet mask, and new subnet mask.

|  |  |
| --- | --- |
| Given: | |
| **Host IP Address:** | 192.168.200.139 |
| **Original Subnet Mask** | 255.255.255.0 |
| **New Subnet Mask:** | 255.255.255.224 |

| Find: | |
| --- | --- |
| **Number of Subnet Bits** | 27-24 = 3 |
| **Number of Subnets Created** | 2^3 = 8 |
| **Number of Host Bits per Subnet** | 32 – 27 = 5 |
| **Number of Hosts per Subnet** | 2^5 – 2 = 30 |
| **Network Address of this Subnet** | 192.168.200.128 |
| **IPv4 Address of First Host on this Subnet** | 192.168.200.129 |
| **IPv4 Address of Last Host on this Subnet** | 192.168.200.158 |
| **IPv4 Broadcast Address on this Subnet** | 192.168.200.159 |

|  |  |
| --- | --- |
| Given: | |
| **Host IP Address:** | 10.101.99.228 |
| **Original Subnet Mask** | 255.0.0.0 |
| **New Subnet Mask:** | 255.255.128.0 |

| Find: | |
| --- | --- |
| **Number of Subnet Bits** | 17-8 = 9 |
| **Number of Subnets Created** | 2^9 = 512 |
| **Number of Host Bits per Subnet** | 32- 17 = 15 |
| **Number of Hosts per Subnet** | 2^15 – 2 = 32,766 |
| **Network Address of this Subnet** | 10.101.0.0 |
| **IPv4 Address of First Host on this Subnet** | 10.101.0.1 |
| **IPv4 Address of Last Host on this Subnet** | 10.101.127.254 |
| **IPv4 Broadcast Address on this Subnet** | 10.101.127.255 |

|  |  |
| --- | --- |
| Given: | |
| **Host IP Address:** | 172.22.32.12 |
| **Original Subnet Mask** | 255.255.0.0 |
| **New Subnet Mask:** | 255.255.224.0 |

| Find: | |
| --- | --- |
| **Number of Subnet Bits** | 19-16 = 3 |
| **Number of Subnets Created** | 2^3 = 8 |
| **Number of Host Bits per Subnet** | 32-19 = 13 |
| **Number of Hosts per Subnet** | 2^13 – 2 = 8,190 |
| **Network Address of this Subnet** | 172.22.32.0 |
| **IPv4 Address of First Host on this Subnet** | 172.22.32.1 |
| **IPv4 Address of Last Host on this Subnet** | 172.22.63.254 |
| **IPv4 Broadcast Address on this Subnet** | 172.22.63.255 |

|  |  |
| --- | --- |
| Given: | |
| **Host IP Address:** | 192.168.1.245 |
| **Original Subnet Mask** | 255.255.255.0 |
| **New Subnet Mask:** | 255.255.255.252 |

| Find: | |
| --- | --- |
| **Number of Subnet Bits** | 30-24 = 6 |
| **Number of Subnets Created** | 2^6 = 64 |
| **Number of Host Bits per Subnet** | 32 – 30 = 2 |
| **Number of Hosts per Subnet** | 2^2 – 2 = 2 |
| **Network Address of this Subnet** | 192.168.1.244 |
| **IPv4 Address of First Host on this Subnet** | 192.168.1.245 |
| **IPv4 Address of Last Host on this Subnet** | 192.168.1.246 |
| **IPv4 Broadcast Address on this Subnet** | 192.168.1.247 |

|  |  |
| --- | --- |
| Given: | |
| **Host IP Address:** | 128.107.0.55 |
| **Original Subnet Mask** | 255.255.0.0 |
| **New Subnet Mask:** | 255.255.255.0 |

| Find: | |
| --- | --- |
| **Number of Subnet Bits** | 24-16 = 8 |
| **Number of Subnets Created** | 2^8 = 256 |
| **Number of Host Bits per Subnet** | 32 – 24 = 8 |
| **Number of Hosts per Subnet** | 2^8 – 2 = 254 |
| **Network Address of this Subnet** | 128.107.0.0 |
| **IPv4 Address of First Host on this Subnet** | 128.107.0.1 |
| **IPv4 Address of Last Host on this Subnet** | 128.107.0.254 |
| **IPv4 Broadcast Address on this Subnet** | 128.107.0.255 |

|  |  |
| --- | --- |
| Given: | |
| **Host IP Address:** | 192.135.250.180 |
| **Original Subnet Mask** | 255.255.255.0 |
| **New Subnet Mask:** | 255.255.255.248 |

| Find: | |
| --- | --- |
| **Number of Subnet Bits** | 29-24 = 5 |
| **Number of Subnets Created** | 2^5 = 32 |
| **Number of Host Bits per Subnet** | 32-29 = 3 |
| **Number of Hosts per Subnet** | 2^3 -2 = 6 |
| **Network Address of this Subnet** | 192.135.250.176 |
| **IPv4 Address of First Host on this Subnet** | 192.135.250.177 |
| **IPv4 Address of Last Host on this Subnet** | 192.135.250.182 |
| **IPv4 Broadcast Address on this Subnet** | 192.135.250.183 |

# Reflection Question

Why is the subnet mask so important when analyzing an IPv4 address?

Type your answers here.

The subnet mask determines everything about the address: the network, number of host bits, number of hosts and the broadcast address.

End of Document

End of document